{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Produkter"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Produkter","index":0,"n_rows":26,"n_cols":10,"rows_kept":26,"cut":false,"hidden":false,"merged":[]}
["Produkt","Licensnummer","Miljömärkning","Kategori","Produktgrupp","Kriteriegeneration","Varumärke","Licensinnehavare","Adress","Ort"]
["9.6mm Bofelle® 3-Layer Wood Floor Bofelle® 138 Oak Lively Soft White MattPro, brushed, 2-side bevelled Toplayer ca. 1,2mm, 5G Dry Click 9.6 x 138 x 2200mm, FSC® Mix credit","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["9.6mm Bofelle® 3-Layer Wood Floor Bofelle® 138 Oak Calm Transparent MattPro, brushed, 2-side bevelled Toplayer ca. 1,2mm, 5G Dry Click 9.6 x 138 x 2200mm, FSC® Mix credit","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["9.6mm Bofelle® 3-Layer Wood Floor Bofelle® 138 Oak Lively Transparent MattPro, brushed, 2-side bevelled Toplayer ca. 1,2mm, 5G Dry Click 9.6 x 138 x 2200mm, FSC® Mix credit","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["9.6mm Bofelle® 3-Layer Wood Floor Bofelle® 138 Oak Lively Soft Brown MattPro, brushed, 2-side bevelled Toplayer ca. 1,2mm, 5G Dry Click 9.6 x 138 x 2200mm, FSC® Mix credit","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["9.6mm Bofelle® 3-Layer Wood Floor Bofelle® 138 Oak  Rustic Transparent MattPro, brushed, 2-side bevelled Toplayer ca. 1,2mm, 5G Dry Click 9.6 x 138 x 2200mm, FSC® Mix credit","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["9.6mm Bofelle® 3-Layer Wood Floor Bofelle® 181 Oak Rustic Authentic MattPro, brushed, 2-side bevelled Toplayer ca. 1,2mm, 5G Dry Click 9.6 x 181 x 2200mm, FSC® Mix credit","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["9.6mm Bofelle® 3-Layer Wood Floor Bofelle® 181 Oak Rustic Soft Brown MattPro, brushed, 2-side bevelled Toplayer ca. 1,2mm, 5G Dry Click 9.6 x 181 x 2200mm, FSC® Mix credit","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["9.6mm Bofelle® 3-Layer Wood Floor Bofelle® 181 Oak Rustic Soft White MattPro, brushed, 2-side bevelled Toplayer ca. 1,2mm, 5G Dry Click 9.6 x 181 x 2200mm, FSC® Mix credit","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["9.6mm Bofelle® 3-Layer Wood Floor Bofelle® 181 Oak Lively Authentic MattPro, brushed, 2-side bevelled Toplayer ca. 1,2mm, 5G Dry Click 9.6 x 181 x 2200mm, FSC® Mix credit","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["9.6mm Bofelle® 3-Layer Wood Floor Bofelle® 209 Oak Lively Authentic MattPro, brushed, 2-side bevelled Toplayer ca. 1,2mm, 5G Dry Click 9.6 x 209 x 2200mm, FSC® Mix Credit","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["9.6mm Bofelle® 3-Layer Wood Floor Bofelle® 209 Oak Rustic Soft White MattPro, brushed, 2-side bevelled Toplayer ca. 1,2mm, 5G Dry Click 9.6 x 209 x 2200mm, FSC® Mix Credit","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["9.6mm Bofelle® 3-Layer Wood Floor Bofelle® 209 Oak Rustic Soft Brown MattPro, brushed, 2-side bevelled Toplayer ca. 1,2mm, 5G Dry Click 9.6 x 209 x 2200mm, FSC® Mix Credit","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["9.6mm Bofelle® 3-Layer Wood Floor Bofelle® 209 Oak Rustic Authentic MattPro, brushed, 2-side bevelled Toplayer ca. 1,2mm, 5G Dry Click 9.6 x 209 x 2200mm, FSC® Mix Credit","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["Bofelle® 181 Ek Soft Brown Lively borstad, 2-sidig fas 5G Dry Click, Y2 9.6 x 181 x 2200 mm, Toppskikt (mm): 1.2 mm","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["Bofelle® 181 Ek Soft White Lively borstad, 2-sidig fas 5G Dry Click, Y2 9.6 x 181 x 2200 mm, Toppskikt (mm): 1.2 mm","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["Bofelle® 181 Ek Transparent Calm borstad, 2-sidig fas 5G Dry Click, Y2 9.6 x 181 x 2200 mm, Toppskikt (mm): 1.2 mm","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["Bofelle® 181 Ek Transparent Lively borstad, 2-sidig fas 5G Dry Click, Y2 9.6 x 181 x 2200 mm, Toppskikt (mm): 1.2 mm","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["Bofelle® 181 Ek Transparent Rustic borstad, 2-sidig fas 5G Dry Click, Y2 9.6 x 181 x 2200 mm, Toppskikt (mm): 1.2 mm","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["Bofelle® 209 Ek Soft Brown Lively borstad, 2-sidig fas 5G Dry Click, Y2 9.6 x 209 x 2200 mm, Toppskikt (mm): 1.2 mm","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["Bofelle® 209 Ek Soft White Lively borstad, 2-sidig fas 5G Dry Click, Y2 9.6 x 209 x 2200 mm, Toppskikt (mm): 1.2 mm","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["Bofelle® 209 Ek Transparent Calm djupborstad, 2-sidig fas 5G Dry Click, Y2 9.6 x 209 x 2200 mm, Toppskikt (mm): 1.2 mm","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["Bofelle® 209 Ek Transparent Lively borstad, 2-sidig fas 5G Dry Click, Y2 9.6 x 209 x 2200 mm, Toppskikt (mm): 1.2 mm","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["Bofelle® 209 Ek Transparent Rustic borstad, 2-sidig fas 5G Dry Click, Y2 9.6 x 209 x 2200 mm, Toppskikt (mm): 1.2 mm","2029 0030, 2029 0029","Svanen","Trägolv","029 Golv","7","BOEN","Bauwerk Group AG","Neudorfstrasse 49","St. Margrethen"]
["Golvabia Maxwood XL Lodge Ek Natur Vit (127034)","3029 0025","Svanen","Trägolv","029 Golv","7","Golvabia","Golvabia AB","Långgatan 10","Anderstorp"]
["Golvabia Maxwood XLW Ek Unique Raw (127137)","3029 0025","Svanen","Trägolv","029 Golv","7","Golvabia","Golvabia AB","Långgatan 10","Anderstorp"]